# Release Notes

# Issues and notes for v2.0.12 2013.08.23

Known issues and notes for version 2.0.12:

2.0.12 - Enhancements/Fixes:

- Fixes from CarDAQ-Plus, VPW and J1708 improved DSP code, _PS on CAN 6 and 14 and J1850.
- added support for J1850 _PS protocols and CAN_PS on 6 and 14.
- Fixed PassThruConnect with a _PS protocol ID did not error if the baudrate was wrong.
- Fixed indication bit of a Single Wire CAN frame with High Voltage was not working.
- Changed hostname from AVIT to CGI_net_name boot option preference.
- Fixed issue with httpd POST method causing hang on CGI read QUERY_STRING.
- Updated Sierra Wireless drivers to version 1.7.40.
- Updated Option HSO packet driver to version 1.14.
- Added /opt/usr/bin to search path for optional installable packages.
- Fixed usb_autorun error the was introduced in early in 2.0.11 betas.
- Added support Option GI1505 Wireless Modem
- ISO15765: Added support for N_Br_MIN and other config parameters.
- J2534-2: Added J1939 Protocol.
- Added sierra serial kernel driver for Sierra Wireless USB 598 and others.
- Added OpenSSH (ssh, sshd, scp, sftp). See AVIT Boot Options for more details.
- ISO15765: PassThruWriteMsgs with a timeout returns an error if a write message failed to transmit.
- ISO15765: removed waiting stmin after a flow control message.
- ISO15765: fixed issue causing 3ms stmin latency.

2.0.10 - Enhancements/Fixes:

- Enhanced FTP security. See AVIT Boot Options for more details.
- Added support for iCON 452 USB Wireless Modem device.
- Increased the maximum number of flow control filters to 32.
- Added support for native gcc compiler and toolchain to be installed on AVIT CF memory card.
- Removed TinyC (tcc) compiler.
- Fixed mixed mode on _PS channel protocol issue.
- Fixed loading of analog calibrations.

2.0.08 - Enhancements/Fixes:

- Fixed battery not trickle charging.
- Added USB autorun feature.
- Fixed hardware reset not working via RESET pinsw command.
- Added support for DrewTech Marvell 8385 CF Module.
- Fixed ISO15765 periodics not working after receiving a segmented message.
- Removed ERR_NO_FLOW_CONTROL return code from PassThruReadMsgs.
- Added J1708_PS_J1939 support, added J1708_PINS support.
- Fixed ISO15765 Pad byte now stored separately for each channel.
- Fixed J1850PWM now allows filters of 1 byte.
- Fixed issue with USBFS not mounting.

2.0.06 - Enhancements/Fixes:

- Added feature to bypass autorun if Wake button is held for greater than 10 seconds at boot.
- Fixed Network LED for Wireless.
- Enabled default colors for ls command.
- Implemented NetPlug for Wireless (Now handles AP changed).
- Fixed issue with vehicle interface locking up system.
- ISO15765 N_As timeout extended.
- Added J2534-2 XXX_SIMULTANEOUS support.
- Implemented NetLink support for CS89x0 Ethernet kernel driver.
- Implemented NetPlug for faster boot times and clean up Ethernet hotplug events.
- Minor changes to init.d files to speed up boot time.
- Fixed console login prompt not being suppressed for "gps_on" condition.
- Fixed issue with date not reading timezone file.