# Release Notes

# Issues and notes for v1.9.18 2009.03.04

Known issues in version 1.9.18:

- "Medium Speed CAN" is implemented as per the J2534-2 spec, although J1962_PINS is optional for now.
- "Single wire CAN" is implemented as per the J2534-2 spec, although J1962_PINS is optional for now.
- "Mixed Format Frames on a CAN Network" (GMLAN) is implemented from the J2534-2 spec, but only for CAN_MIXED_MODE=1.
- The on-board clock cannot be set from web

# Release notes for v1.9.18 2009.03.04

The following fixes have been made in version 1.9.18:

- Fixed VPP control issue when switching SCI protocols after using SCI_TX_VOLTAGE.
- Changed ISO15765 interaction with Periodics to accomidate a Ford issue.
- Added J2534-2 Discovery Mechanism.
- Fixed ISO15765 STmin timer to meet spec. Time between, not start to start.
- Fixed debug log writing to support legacy directory enable.
- Fixed ISO9141 CS error on 24 byte boundaries.
- Improved Multi-thread error detection.

# Release notes for v1.9.16 2008.12.03

The following fixes have been made in version 1.9.16:

- Analog Protocol ID now matches J2534-2 (supports old value too, for now).
- J1708 now matches J2534-2 spec (priority in TxFlags).
- USB now works after closing an Ethernet connection.
- ISO14230 Fast Init now handles NULL parameters correctly.
- CLEAR_RX_BUFFER now gets all messages from driver before clear.
- ISO9141, ISO14230, delay P3_MIN after a break is received.
- Improved debug log name and saves to Logs directory.
- Fixed CLEAR_MSG_FILTERS to not report errors in debug log.
- Added cron and crontab to busy box.
- Added timestamp to Error returns in debug log.
- Installer no longer installs 0202 dll, no longer sets registry for 0202.
- Fixed default calculation of IP address for wireless configuration.